**HP M880 59.00.30 error**

In case anyone else comes across that error it was a fuser drive motor error but the wiring was not sitting correctly so the fuser drive gear was rubbing the wire and removed the coating and was shorting it the wire. Wrapped wire in electrical tape and reseated wiring properly and printer now works perfectly